These are the updated XSVF RGH files for Zephyr, Falcon, Jasper & Trinity to include support for the Demon CR_EN 
feature (CoolRunner Enable/Disable). 

This is needed if you wish to boot a stock (untouched) onboard nand for xbl.

Attached are both sets of RGH1 and RGH2.

This updates all RGH1/RGH2 Phat and Trinity RGH Slim (which is based on RGH2 code). There is no Xenon support for
obvious reasons.

DEMON PHAT RGH2 CoolRunner CR_EN File Info:

Zephyr: Program either RGH2_DEMON_CR_EN_D.xsvf, or RGH2_DEMON_CR_EN_C.xsvf

Falcon/Opus: Program either RGH2_DEMON_CR_EN_B.xsvf, or RGH2_DEMON_CR_EN_C.xsvf

Jasper: Program either RGH2_DEMON_CR_EN_A.xsvf, or RGH2_DEMON_CR_EN_D.xsvf
 

The CoolRunner Rev C already has the CR_EN pad to solder to, however the Rev A and B do not as they are older 
models, however we have designed the new code to use one of the corner pins of the Rev A and Rev B. 

Visit here for more info: http://www.team-xecuter.com/forums/showthread.php?t=88173

Team Xecuter
June 26 2012